Using the TEMD6010X photodiode (providing a nominal 128uA current at 1367W/m^2, 150uA maximum at 3.3V). Beyond 150uA, the output voltage will stay at 3.3V.

